directory 1: /DIRECTORY/SampleDirectory.csv # Points to customer directory

directed call pickup: 1 # enables the directed call pickup prefix 0=Disable, 1=Enable

directed call pickup prefix: 00 # Sets the directed call pickup prefix

auto resync mode: 0 # 0=Disable, 1=Enable

call waiting tone: 0 # 0=Disable, 1=Enable

collapsed more softkey screen: 1 # 0=Disable, 1=Enable

missed calls indicator disabled: 1 # 0=False, 1=True

blf display label to max: 1 # 0=Primary, 1=Secondary Specifies how the phone truncates BLF and BLF/List softkey labels.

sip intercom allow barge in: 0 # 0=Does NOT allow barge in 1=Does allow barge-in

# Top Buttons for top of display

topsoftkey1 type: speeddial

topsoftkey1 label: VoiceMail

topsoftkey1 value: \*98

topsoftkey4 type: blf

topsoftkey4 label: Park

topsoftkey4 value: 700

# Bottom Buttons for bottom of display

softkey1 type: blf

softkey1 label: Phone 101

softkey1 value: 101

softkey2 type: blf

softkey2 label: Phone 102

softkey2 value: 102

softkey3 type: blf

softkey3 label: Phone 103

softkey3 value: 103

softkey4 type: blf

softkey4 label: Phone 104

softkey4 value: 104

softkey5 type: blf

softkey5 label: Phone 105

softkey5 value: 105

softkey6 type: blf

softkey6 label: Phone 106

softkey6 value: 106