remote\_phonebook.data.1.url = http://config.ivscomm.com/DIRECTORY/Sample.xml

remote\_phonebook.data.1.name = Sample

## Tones for when you dial 0=disabled 1=Enabled ##

features.key\_tone = 0

## Dialog popup on screen for missed calls 0=disabled 1=Enabled ##

features.missed\_call\_popup.enable = 0

## Stop the power LED from blinking like you have a voicemail, especially useful for places that ring all phones first (S series phones only!)

phone\_setting.missed\_call\_power\_led\_flash.enable = 0

phone\_setting.mail\_power\_led\_flash\_enable = 1

## Stops the ghost calls

features.direct\_ip\_call\_enable=0

sip.trust\_ctrl=1

##transfer caller ID

account.1.refresh\_remote\_id.enable = 1

##enable browser control of phone

features.action\_uri\_limit\_ip=any

features.show\_action\_uri\_option=0

ActionURIShowMsgBox = 0

###Paging Settings

multicast.receive\_priority.enable = 0

multicast.receive\_priority.priority = 0

multicast.listen\_address.30.label = Paging All

multicast.listen\_address.30.ip\_address = 224.0.0.2:10000

multicast.listen\_address.30.channel = 30

multicast.codec = PCMU

programablekey.3.type = 24

programablekey.3.line = 1

programablekey.3.extension = 30

programablekey.3.value = 224.0.0.2:10000

programablekey.3.label = Page All

programablekey.3.xml\_phonebook = 0

## sip.timer\_t1 = 2

##sip session timer edit to longer than default timeout

## DO NOT CHANGE OR OMIT THE FIRST THREE BUTTONS ##

linekey.1.type = 15

linekey.1.line = 1

linekey.1.label = Line 1

linekey.2.type = 15

linekey.2.line = 1

linekey.2.label = Line 2

linekey.3.type = 13

linekey.3.line = 1

linekey.3.value = 700

linekey.3.label = Park

######################

linekey.4.type = 16

linekey.4.line = 1

linekey.4.value = 101

linekey.4.label = 101

linekey.5.type = 16

linekey.5.line = 1

linekey.5.value = 102

linekey.5.label = 102

linekey.6.type = 16

linekey.6.line = 1

linekey.6.value = 103

linekey.6.label = 103